/**
  @page PWR_SLEEP Power sleep Mode Example
  
  @verbatim
  ******************** (C) COPYRIGHT 2016 STMicroelectronics *******************
  * @file    PWR/PWR_SLEEP/readme.txt 
  * @author  MCD Application Team
  * @version V1.5.0
  * @date    14-April-2017
  * @brief   Description of the Power Sleep Mode example.
  ******************************************************************************
  *
  * Redistribution and use in source and binary forms, with or without modification,
  * are permitted provided that the following conditions are met:
  *   1. Redistributions of source code must retain the above copyright notice,
  *      this list of conditions and the following disclaimer.
  *   2. Redistributions in binary form must reproduce the above copyright notice,
  *      this list of conditions and the following disclaimer in the documentation
  *      and/or other materials provided with the distribution.
  *   3. Neither the name of STMicroelectronics nor the names of its contributors
  *      may be used to endorse or promote products derived from this software
  *      without specific prior written permission.
  *
  * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
  * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
  * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
  * DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE
  * FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
  * DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
  * SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
  * CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY,
  * OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
  * OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
  @endverbatim

@par Example Description 

How to enter the Sleep mode and wake up from this mode by using an interrupt.

In the associated software, the system clock is set to 24 MHz, the SysTick is 
programmed to generate an interrupt each 1 ms.

In the associated software
  - the system clock is set to 24 MHz.
  - EXTI_Line0 is configured to generate an interrupt on falling edge.
  - the SysTick is programmed to generate an interrupt each 1 ms. 

The system enters SLEEP mode after 5 seconds and will wait for the User push-button is pressed
to wake up from SLEEP mode. Current consumption could be monitored through an amperemeter.

This behavior is repeated in an infinite loop.

    - SLEEP Mode
    =======================
          - System Running at 24 MHz
          - Code running from Internal FLASH
          - All peripherals OFF
          - Wakeup using EXTI Line (User push-button PA.00)

@note This example can not be used in DEBUG mode, this is due to the fact 
      that the Cortex-M3 core is no longer clocked during low power mode 
       so debugging features are disabled

@note Care must be taken when using HAL_Delay(), this function provides accurate delay (in milliseconds)
      based on variable incremented in SysTick ISR. This implies that if HAL_Delay() is called from
      a peripheral ISR process, then the SysTick interrupt must have higher priority (numerically lower)
      than the peripheral interrupt. Otherwise the caller ISR process will be blocked.
      To change the SysTick interrupt priority you have to use HAL_NVIC_SetPriority() function.
      
@note The application need to ensure that the SysTick time base is always set to 1 millisecond
      to have correct HAL operation.
      
@par Directory contents 

  - PWR/PWR_SLEEP/Inc/stm32f1xx_conf.h         HAL Configuration file
  - PWR/PWR_SLEEP/Inc/stm32f1xx_it.h           Header for stm32f1xx_it.c
  - PWR/PWR_SLEEP/Inc/main.h                   Header file for main.c
  - PWR/PWR_SLEEP/Src/system_stm32f1xx.c       STM32F1xx system clock configuration file
  - PWR/PWR_SLEEP/Src/stm32f1xx_it.c           Interrupt handlers
  - PWR/PWR_SLEEP/Src/main.c                   Main program

@par Hardware and Software environment

  - This example runs on STM32F1xx devices
      
  - This example has been tested with STMicroelectronics STM32VL-Discovery
    evaluation board and can be easily tailored to any other supported device 
    and development board.

  - STM32VL-Discovery Set-up
    - Use the User push-button connected to pin PA.00 (EXTI_Line0)
    - Connect an amperemeter to JP1 to measure the IDD current

@par How to use it ? 

In order to make the program work, you must do the following :
 - Open your preferred toolchain 
 - Rebuild all files and load your image into target memory
 - Run the example


 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
