/**
  @page SPI_TwoBoards_FullDuplex_IT SPI example
  
  @verbatim
  ******************** (C) COPYRIGHT 2016 STMicroelectronics *******************
  * @file    Examples_LL/SPI/SPI_TwoBoards_FullDuplex_IT/readme.txt 
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    14-April-2017
  * @brief   Description of the SPI_TwoBoards_FullDuplex_IT example.
  ******************************************************************************
  *
  * Redistribution and use in source and binary forms, with or without modification,
  * are permitted provided that the following conditions are met:
  *   1. Redistributions of source code must retain the above copyright notice,
  *      this list of conditions and the following disclaimer.
  *   2. Redistributions in binary form must reproduce the above copyright notice,
  *      this list of conditions and the following disclaimer in the documentation
  *      and/or other materials provided with the distribution.
  *   3. Neither the name of STMicroelectronics nor the names of its contributors
  *      may be used to endorse or promote products derived from this software
  *      without specific prior written permission.
  *
  * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
  * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
  * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
  * DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE
  * FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
  * DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
  * SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
  * CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY,
  * OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
  * OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
  @endverbatim

@par Example Description 

Data buffer transmission and receptionvia SPI using Interrupt mode. This 
example is based on the STM32F1xx SPI LL API. The peripheral 
initialization uses LL unitary service functions for optimization purposes (performance and size).

The communication is done with 2 boards through SPI.
   _________________________                        _________________________
  |       ___________ ______|                      |__________________       |
  |      |SPI1              |                      |             SPI1 |      |
  |      |                  |                      |                  |      |
  |      |        CLK(PB13) |______________________|(PB13)CLK         |      |
  |      |                  |                      |                  |      |
  |      |        MISO(PB14)|______________________|(PB14)MISO        |      |
  |      |                  |                      |                  |      |
  |      |        MOSI(PB15)|______________________|(PB15)MOSI        |      |
  |      |                  |                      |                  |      |
  |      |__________________|                      |__________________|      |
  |      __                 |                      |                         |
  |     |__|                |                      |                         |
  |     USER                |                      |                         |
  |                      GND|______________________|GND                      |
  |                         |                      |                         |
  |_STM32F1xx Master _______|                      |_STM32F1xx Slave ________|

This example shows how to configure GPIO and SPI peripherals
to use a Full-Duplex communication using IT mode through the STM32F1xx COM_INSTANCE1_TYPE LL API.

The project is splitted in two parts the Master Board and the Slave Board:

- Master Board
  SPI1 Peripheral is configured in Master mode.
  SPI1_IRQn activated. 
  RXNE and TXE Interrupts SPI peripheral activated.
  GPIO associated to User push-button is linked with EXTI. 
  
- Slave Board
  SPI1 Peripheral is configured in Slave mode.
  SPI1_IRQn activated. 
  RXNE and TXE Interrupts SPI peripheral activated.

The user can choose between Master and Slave through "#define MASTER_BOARD"
in the "main.c" file:
- Uncomment "#define MASTER_BOARD" to select Master board.
- Comment "#define MASTER_BOARD" to select Slave board.

Example execution:
On BOARD MASTER, LED2 is blinking Fast (200ms) and wait User push-button action.
Press User push-button on BOARD MASTER start a Full-Duplex communication through IT.
On MASTER side, Clock will be generated on SCK line, Transmission(MOSI Line) and reception (MISO Line) 
will be done at the same time. 
SLAVE SPI will received  the Clock (SCK Line), so Transmission(MISO Line) and reception (MOSI Line) will be done also.

LED2 is On if data is well received.

In case of errors, LED2 is blinking Slowly (1s).

@note You need to perform a reset on Master board, then perform it on Slave board
      to have the correct behaviour of this example.


@par Directory contents 

  - SPI/SPI_TwoBoards_FullDuplex_IT/Inc/stm32f1xx_it.h          Interrupt handlers header file
  - SPI/SPI_TwoBoards_FullDuplex_IT/Inc/main.h                  Header for main.c module
  - SPI/SPI_TwoBoards_FullDuplex_IT/Inc/stm32_assert.h          Template file to include assert_failed function
  - SPI/SPI_TwoBoards_FullDuplex_IT/Src/stm32f1xx_it.c          Interrupt handlers
  - SPI/SPI_TwoBoards_FullDuplex_IT/Src/main.c                  Main program
  - SPI/SPI_TwoBoards_FullDuplex_IT/Src/system_stm32f1xx.c      STM32F1xx system source file

@par Hardware and Software environment

  - This example runs on STM32F103xB devices.

  - This example has been tested with STM32F103RB-Nucleo board and can be
    easily tailored to any other supported device and development board.

  - STM32F103RB-Nucleo Set-up
    - Connect Master board PB13 to Slave Board PB13 (connected to pin 30 of CN10 connector)
    - Connect Master board PB14 to Slave Board PB14 (connected to pin 28 of CN10 connector)
    - Connect Master board PB15 to Slave Board PB15 (connected to pin 26 of CN10 connector)
    - Connect Master board GND to Slave Board GND

@par How to use it ? 

In order to make the program work, you must do the following :
 - Open your preferred toolchain
 - Rebuild all files and load your image into target memory
    o Uncomment "#define MASTER_BOARD" and load the project in Master Board
    o Comment "#define MASTER_BOARD" and load the project in Slave Board
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
