Back to Release page
# Release Notes for STM32F1xx_Nucleo Board Drivers Copyright 2016 STMicroelectronics
## Contents STM32F1xx_Nucleo Board Drivers update History License ## STM32F1xx_Nucleo Board Drivers update History ### V1.0.4 / 14-April-2017 Main Changes Add STM32F1xx_Nucleo_BSP_User_Manual.chm file ### V1.0.3 / 29-April-2016 Main Changes Add support for 4 Gb sd cards. ### V1.0.2 / 18-December-2015 Main Changes Add an alias from BUTTON_KEY to BUTTON_USER for compatibility with STM32F4xx and STM32L0xx. BSP_LED_Init: Configure the led in GPIO_NOPULL instead of GPIO_PULLUP to reduce power consumption. Rename GPIO_SPEED_HIGH to GPIO_SPEED_FREQ_HIGH for compatibility with STM32F1xx HAL Drivers V1.0.2. Rename GPIO_SPEED_MEDIUM to GPIO_SPEED_FREQ_MEDIUM for compatibility with STM32F1xx HAL Drivers V1.0.2. ### V1.0.1 / 31-July-2015 Main Changes Add ADC calibration for JoyStick management. Improve the polling of ADC in BSP_JOY_GetState. ### V1.0.0 / 15-December-2014 Main Changes Official release for STM32F1xx_Nucleo board RevC drivers for STM32Cube_FW_F1 project ## License Licensed under MCD-ST Liberty SW License Agreement V2, (the "License"); You may not use this package except in compliance with the License. You may obtain a copy of the License at: http://www.st.com/software_license_agreement_liberty_v2 Unless required by applicable law or agreed to in writing, software distributed under the License is distributed on an "AS IS" BASIS, WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied. See the License for the specific language governing permissions and limitations under the License. For complete documentation on STM32 Microcontrollers visit www.st.com/STM32