CMSIS-CORE: SCB_Type Struct Reference

| CMSIS-CORE Version 4.30 CMSIS-CORE support for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Fields

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Data Fields
SCB_Type Struct Reference

Structure type to access the System Control Block (SCB).

## Data Fields
__IM uint32_t | CPUID
| Offset: 0x000 (R/ ) CPUID Base Register.
__IOM uint32_t | ICSR
| Offset: 0x004 (R/W) Interrupt Control and State Register.
__IOM uint32_t | VTOR
| Offset: 0x008 (R/W) Vector Table Offset Register.
__IOM uint32_t | AIRCR
| Offset: 0x00C (R/W) Application Interrupt and Reset Control Register.
__IOM uint32_t | SCR
| Offset: 0x010 (R/W) System Control Register.
__IOM uint32_t | CCR
| Offset: 0x014 (R/W) Configuration Control Register.
__IOM uint8_t | SHP [12]
| Offset: 0x018 (R/W) System Handlers Priority Registers (4-7, 8-11, 12-15)
__IOM uint32_t | SHCSR
| Offset: 0x024 (R/W) System Handler Control and State Register.
__IOM uint32_t | CFSR
| Offset: 0x028 (R/W) Configurable Fault Status Register.
__IOM uint32_t | HFSR
| Offset: 0x02C (R/W) HardFault Status Register.
__IOM uint32_t | DFSR
| Offset: 0x030 (R/W) Debug Fault Status Register.
__IOM uint32_t | MMFAR
| Offset: 0x034 (R/W) MemManage Fault Address Register.
__IOM uint32_t | BFAR
| Offset: 0x038 (R/W) BusFault Address Register.
__IOM uint32_t | AFSR
| Offset: 0x03C (R/W) Auxiliary Fault Status Register.
__IM uint32_t | PFR [2]
| Offset: 0x040 (R/ ) Processor Feature Register.
__IM uint32_t | DFR
| Offset: 0x048 (R/ ) Debug Feature Register.
__IM uint32_t | ADR
| Offset: 0x04C (R/ ) Auxiliary Feature Register.
__IM uint32_t | MMFR [4]
| Offset: 0x050 (R/ ) Memory Model Feature Register.
__IM uint32_t | ISAR [5]
| Offset: 0x060 (R/ ) Instruction Set Attributes Register.
uint32_t | RESERVED0 [5]
| Reserved.
__IOM uint32_t | CPACR
| Offset: 0x088 (R/W) Coprocessor Access Control Register.

## Field Documentation

__IM uint32_t SCB_Type::ADR

__IOM uint32_t SCB_Type::AFSR

__IOM uint32_t SCB_Type::AIRCR

__IOM uint32_t SCB_Type::BFAR

__IOM uint32_t SCB_Type::CCR

__IOM uint32_t SCB_Type::CFSR

__IOM uint32_t SCB_Type::CPACR

__IM uint32_t SCB_Type::CPUID

__IM uint32_t SCB_Type::DFR

__IOM uint32_t SCB_Type::DFSR

__IOM uint32_t SCB_Type::HFSR

__IOM uint32_t SCB_Type::ICSR

__IM uint32_t SCB_Type::ISAR[5]

__IOM uint32_t SCB_Type::MMFAR

__IM uint32_t SCB_Type::MMFR[4]

__IM uint32_t SCB_Type::PFR[2]

uint32_t SCB_Type::RESERVED0[5]

__IOM uint32_t SCB_Type::SCR

__IOM uint32_t SCB_Type::SHCSR

__IOM uint8_t SCB_Type::SHP[12]

__IOM uint32_t SCB_Type::VTOR