CMSIS-CORE: TPI_Type Struct Reference

| CMSIS-CORE Version 4.30 CMSIS-CORE support for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

- Data Structures
- Data Fields

All Data Structures Files Functions Variables Enumerations Enumerator Groups Pages
Data Fields
TPI_Type Struct Reference

Structure type to access the Trace Port Interface Register (TPI).

## Data Fields
__IOM uint32_t | SSPSR
| Offset: 0x000 (R/ ) Supported Parallel Port Size Register.
__IOM uint32_t | CSPSR
| Offset: 0x004 (R/W) Current Parallel Port Size Register.
uint32_t | RESERVED0 [2]
| Reserved.
__IOM uint32_t | ACPR
| Offset: 0x010 (R/W) Asynchronous Clock Prescaler Register.
uint32_t | RESERVED1 [55]
| Reserved.
__IOM uint32_t | SPPR
| Offset: 0x0F0 (R/W) Selected Pin Protocol Register.
uint32_t | RESERVED2 [131]
| Reserved.
__IM uint32_t | FFSR
| Offset: 0x300 (R/ ) Formatter and Flush Status Register.
__IOM uint32_t | FFCR
| Offset: 0x304 (R/W) Formatter and Flush Control Register.
__IM uint32_t | FSCR
| Offset: 0x308 (R/ ) Formatter Synchronization Counter Register.
uint32_t | RESERVED3 [759]
| Reserved.
__IM uint32_t | TRIGGER
| Offset: 0xEE8 (R/ ) TRIGGER.
__IM uint32_t | FIFO0
| Offset: 0xEEC (R/ ) Integration ETM Data.
__IM uint32_t | ITATBCTR2
| Offset: 0xEF0 (R/ ) ITATBCTR2.
uint32_t | RESERVED4 [1]
| Reserved.
__IM uint32_t | ITATBCTR0
| Offset: 0xEF8 (R/ ) ITATBCTR0.
__IM uint32_t | FIFO1
| Offset: 0xEFC (R/ ) Integration ITM Data.
__IOM uint32_t | ITCTRL
| Offset: 0xF00 (R/W) Integration Mode Control.
uint32_t | RESERVED5 [39]
| Reserved.
__IOM uint32_t | CLAIMSET
| Offset: 0xFA0 (R/W) Claim tag set.
__IOM uint32_t | CLAIMCLR
| Offset: 0xFA4 (R/W) Claim tag clear.
uint32_t | RESERVED7 [8]
| Reserved.
__IM uint32_t | DEVID
| Offset: 0xFC8 (R/ ) TPIU_DEVID.
__IM uint32_t | DEVTYPE
| Offset: 0xFCC (R/ ) TPIU_DEVTYPE.

## Field Documentation

__IOM uint32_t TPI_Type::ACPR

__IOM uint32_t TPI_Type::CLAIMCLR

__IOM uint32_t TPI_Type::CLAIMSET

__IOM uint32_t TPI_Type::CSPSR

__IM uint32_t TPI_Type::DEVID

__IM uint32_t TPI_Type::DEVTYPE

__IOM uint32_t TPI_Type::FFCR

__IM uint32_t TPI_Type::FFSR

__IM uint32_t TPI_Type::FIFO0

__IM uint32_t TPI_Type::FIFO1

__IM uint32_t TPI_Type::FSCR

__IM uint32_t TPI_Type::ITATBCTR0

__IM uint32_t TPI_Type::ITATBCTR2

__IOM uint32_t TPI_Type::ITCTRL

uint32_t TPI_Type::RESERVED0[2]

uint32_t TPI_Type::RESERVED1[55]

uint32_t TPI_Type::RESERVED2[131]

uint32_t TPI_Type::RESERVED3[759]

uint32_t TPI_Type::RESERVED4[1]

uint32_t TPI_Type::RESERVED5[39]

uint32_t TPI_Type::RESERVED7[8]

__IOM uint32_t TPI_Type::SPPR

__IOM uint32_t TPI_Type::SSPSR

__IM uint32_t TPI_Type::TRIGGER