{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":76,"n_cols":8,"rows_kept":76,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Контакт","Сигнал","Наименование DEC","нумерация DEC","Описание","Наименование сигнала","Альтернативное наименование"]
["А:А1","К ТПР5 Н","B IRQ5 L","AA1","Запрос прерывания с приоритетом 5"]
["А:А2","К ТПР6 Н","B IRQ6 L","AB1","Запрос прерывания с приоритетом 6"]
["А:А3","К А16 Н","B DA16 L","AC1","Адрес",null,"A16"]
["А:А4","К А17 Н","B DA17","AD1","Адрес",null,"A17"]
["А:А5","РПА","S SPARE1","AE1","Резерв S1"]
["А:А6","У ОЗУ","S SPARE2","AF1","Резерв S2"]
["А:А7","И ОСТ Н\nSEL","S SPARE3","AH1","вывод с проца HLTM\nSEL",null,"ВА7\nАА7","* SEL это допфункция для какой-то иной корзины"]
["А:А8","ОБЩ","GND","AJ1","общий","GND","общий"]
["А:А9","ОТЛ1","M SPAREA1","AK1","Резерв М А1"]
["А:А10","ОТЛ1","M SPAREB1","AL1","Резерв М B1"]
["А:А11","ОБЩ","GND","AM1","общий","GND","общий"]
["А:А12","К ТПД Н","B DMR L","AN1","Требование прямого доступа (запрос к магистрали)"]
["А:А13","К ОСТ Н","B HALT L","AP1","Останов","HALT","ОСТ"]
["А:А14","К РГН Н","B REF L","AR1","Регенерация памяти","REF","РГН"]
["А:А15","ПРЕЗ1","+12VB","AS1","питание от батареи +12В"]
["А:А16","ОБЩ","GND","AT1","общий"]
["А:А17","ПРЕЗ2","P SPARE1","AU1","Резерв P 1"]
["А:А18","+5ВБ","+5VB","AV1","питание от батареи +5В","питание","питание"]
[]
["Б:А1","К ПОСТН В","B DCOK H","BA1","Постоянное напряжение нормальное (авария источника питания)","DCOK","АИП"]
["Б:А2","К ПИТН В","B POK H","BB1","Сетевое питание нормальное (авария сетевого питания)","POK","АСП"]
["Б:А3","К А18 Н","B DA18 L","BC1","Адрес",null,"A18"]
["Б:А4","К А19 Н","B DA19 L","BD1","Адрес",null,"A19"]
["Б:А5","К А20 Н","B DA20 L","BE1","Адрес",null,"A20"]
["Б:А6","К А21 Н","B DA21 L","BF1","Адрес",null,"A21"]
["Б:А7","Рез8","S SPARE8","BH1","Резерв S8"]
["Б:А8","Общ","GND","BJ1","общий","GND","общий"]
["Б:А9","ОТЛ2","M SPAREA2","BK1","Резерв М А2"]
["Б:А10","ОТЛ2","M SPAREB2","BL1","Резерв М B3"]
["Б:А11","Общ","GND","BM1","общий","GND","общий"]
["Б:А12","К ПВ Н","B SACK L","BN1","Подтверждение выборки(запроса) системного канала(магистрали)","SACK","ПЗ"]
["Б:А13","К ТПР7 Н","B IRQ7 L","BP1","Запрос прерывания с приоритетом 7",null,null,"?"]
["Б:А14","X","B EVNT L","BR1","Прерывание по таймеру (внешнему событию)","EVNT","ПВС"]
["Б:А15","ПРЕЗ3","+12VB","BS1","питание от батареи +12В"]
["Б:А16","Общ","GND","BT1","общий","GND","общий"]
["Б:А17","През4","P SPARE2","BU1","Резерв P 2"]
["Б:А18","+5В","+5V","BV1","питание","питание","питание"]
[]
["А:Б1","+5В","+5V","AA2","питание","питание","питание"]
["А:Б2","-12В","-12V","AB2","питание","питание","питание"]
["А:Б3","Общ","GND","AC2","общий","GND","общий"]
["А:Б4","+12В","+12V","AD2","питание","питание","питание"]
["А:Б5","К ВЫВОД Н","B DOUT L","AE2","Вывод(запись) данных","DOUT","ДЗП"]
["А:Б6","К СИП Н","B RPLY L","AF2","Ответ пассивного устройства","RPLY","ОТВ"]
["А:Б7","К ВВОД Н","B DIN L","AH2","Ввод(чтение) данных","DIN","ДЧТ"]
["А:Б8","К СИА Н","B SYNC L","AJ2","Синхронизация активного устройства","SYNC","ОБМ"]
["А:Б9","К Байт Н","B WTBT L","AK2","Выбор (признак записи) байта","WTBT","ПЗП"]
["А:Б10","К ТПР4 Н","B IRQ 4 L","AL2","Запрос прерывания с приоритетом 4"]
["А:Б11","К ППРI Н","B IAKI L","AM2","Предоставление (разрещение) прерываний (вход)","IAKI","ПРРI"]
["А:Б12","К ППРO Н","B IAKO L","AN2","Предоставление (разрещение) прерываний (выход)","IAKO","ПРРO"]
["А:Б13","К ВУ Н","B BS7 L","AP2","Выбор внешних устройств","BS7","ВУ"]
["А:Б14","К ППДI Н","B DMGI L","AR2","Предоставление прямого доступа (разрешение захвата магистрали) вход","DMGI","РЗМI"]
["А:Б15","К ППДO Н","B DMGO L","AS2","Предоставление прямого доступа (разрешение захвата магистрали) выход","DMGO","РЗМO"]
["А:Б16","К СБРОС Н","B INIT L","AT2","Начальная установка","INIT","УСТ"]
["А:Б17","К ДА00 Н","B DA0 L","AU2","Адрес-данные","DAL00","АД00"]
["А:Б18","К ДА01 Н","B DA1 L","AV2","Адрес-данные","DAL01","АД01"]
[]
["Б:Б1","+5В","+5","BA2","питание","питание","питание"]
["Б:Б2","-12В","-12","BB2","питание","питание","питание"]
["Б:Б3","Общ","GND","BC2","общий","общий","общий"]
["Б:Б4","+12В","+12","BD2","питание","питание","питание"]
["Б:Б5","К ДА 02 Н","B DA2 L","BE2","Адрес-данные","DA02","АД02"]
["Б:Б6","К ДА 03 Н","B DA3 L","BF2","Адрес-данные","DA03","АД03"]
["Б:Б7","К ДА 04 Н","B DA4 L","BH2","Адрес-данные","DA04","АД04"]
["Б:Б8","К ДА 05 Н","B DA5 L","BJ2","Адрес-данные","DA05","АД05"]
["Б:Б9","К ДА 06 Н","B DA6 L","BK2","Адрес-данные","DA06","АД06"]
["Б:Б10","К ДА 07 Н","B DA7 L","BL2","Адрес-данные","DA07","АД07"]
["Б:Б11","К ДА 08 Н","B DA8 L","BM2","Адрес-данные","DA08","АД08"]
["Б:Б12","К ДА 09 Н","B DA9 L","BN2","Адрес-данные","DA09","АД09"]
["Б:Б13","К ДА 10 Н","B DA10 L","BP2","Адрес-данные","DA10","АД10"]
["Б:Б14","К ДА 11 Н","B DA11 L","BR2","Адрес-данные","DA11","АД11"]
["Б:Б15","К ДА 12 Н","B DA12 L","BS2","Адрес-данные","DA12","АД12"]
["Б:Б16","К ДА 13 Н","B DA13 L","BT2","Адрес-данные","DA13","АД13"]
["Б:Б17","К ДА 14 Н","B DA14 L","BU2","Адрес-данные","DA14","АД14"]
["Б:Б18","К ДА 15 Н","B DA15 L","BV2","Адрес-данные","DA15","АД15"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}