/**
  @page ADC_DMA_Transfer ADC DMA Transfer example

  @verbatim
  ******************** (C) COPYRIGHT 2016 STMicroelectronics *******************
  * @file    ADC/ADC_DMA_Transfer/readme.txt 
  * @author  MCD Application Team
  * @brief   Description of the ADC DMA Transfer example.
  ******************************************************************************
  *
  * Redistribution and use in source and binary forms, with or without modification,
  * are permitted provided that the following conditions are met:
  *   1. Redistributions of source code must retain the above copyright notice,
  *      this list of conditions and the following disclaimer.
  *   2. Redistributions in binary form must reproduce the above copyright notice,
  *      this list of conditions and the following disclaimer in the documentation
  *      and/or other materials provided with the distribution.
  *   3. Neither the name of STMicroelectronics nor the names of its contributors
  *      may be used to endorse or promote products derived from this software
  *      without specific prior written permission.
  *
  * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
  * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
  * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
  * DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE
  * FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
  * DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
  * SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
  * CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY,
  * OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
  * OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
  @endverbatim

@par Example Description 

This example describes how to configure and use the ADC to convert an external
analog input and get the result using a DMA transfer through the HAL API.

The ADC is configured to convert continuously ADC_CHANNEL_0, resolution is set to 12
bits right aligned, conversion is software-triggered.

DMA1_Channel1 is configured in Circular mode to transfer continuously
the content of ADC_DR (Data Register) to "aADCxConvertedData" variable which 
stores the conversion result.

User may watch variable array "aADCxConvertedData" and check that its values are modified
according to the voltage applied to pin PA.00 (pin 15 in P1 connector).

STM32 board LED can be used to monitor the conversion:
  - LED3 is ON when there is an error in initialization.


@note Care must be taken when using HAL_Delay(), this function provides accurate delay (in milliseconds)
      based on variable incremented in SysTick ISR. This implies that if HAL_Delay() is called from
      a peripheral ISR process, then the SysTick interrupt must have higher priority (numerically lower)
      than the peripheral interrupt. Otherwise the caller ISR process will be blocked.
      To change the SysTick interrupt priority you have to use HAL_NVIC_SetPriority() function.
      
@note The application need to ensure that the SysTick time base is always set to 1 millisecond
      to have correct HAL operation.

@par Directory contents 

  - ADC/ADC_DMA_Transfer/Inc/stm32f0xx_hal_conf.h    HAL configuration file
  - ADC/ADC_DMA_Transfer/Inc/stm32f0xx_it.h          HAL interrupt handlers header file
  - ADC/ADC_DMA_Transfer/Inc/main.h                  Header for main.c module  
  - ADC/ADC_DMA_Transfer/Src/stm32f0xx_it.c          HAL interrupt handlers
  - ADC/ADC_DMA_Transfer/Src/main.c                  Main program
  - ADC/ADC_DMA_Transfer/Src/stm32f0xx_hal_msp.c     HAL MSP file 
  - ADC/ADC_DMA_Transfer/Src/system_stm32f0xx.c      STM32F0xx system source file


@par Hardware and Software environment

  - This example runs on STM32F030x8 devices.

  - This example has been tested with STM32F0308-Discovery RevA board and can be
    easily tailored to any other supported device and development board.

  - STM32F0308-Discovery RevA Set-up
    Use an external power supply and adjust supply voltage and connect it on 

  - To monitor the conversion result, put the "aADCxConvertedData" variable in the debugger live watch.

@par How to use it ?

In order to make the program work, you must do the following :
 - Open your preferred toolchain 
 - Rebuild all files and load your image into target memory
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
