Back to Release page
# Release Notes for STM32F0xx CMSIS Copyright 2016 STMicroelectronics
## Update History ### V2.3.3 / 25-August-2017 Main Changes Remove support of Atollic TrueSTUDIO STM32 (TrueSTUDIO) toolchain. Performance improvement of the startup code for GCC. ### V2.3.2 / 07-April-2017 Main Changes Rename GPIO_AFRH and GPIO_AFRL bitfields for alignment with all STM32 series. Add macro definition : IS_TIM_ADVANCED. Rename RTC_CR register bit definition to be aligned with STM32F0xx Reference Manual : RTC_CR_BCK ==> RTC_CR_BKP ### V2.3.1 / 04-November-2016 Main Changes Add TIM6_IRQHandler in vectors table for STM32F030x8 devices ### V2.3.0 / 27-May-2016 Main Changes General updates Updated CMSIS Device compliancy with MISRA C 2004 rules: MISRA C 2004 rule 10.5 (bitwise operators ~ and <<). MISRA C 2004 rule 10.6 ('U' suffix applied to all constants of 'unsigned' type). U pdated system_stm32f3xx.h/.c files: Added AHBPrescTable definition as external. Added APBPrescTable definition as external. EXTI updates Added definitions of bit 31 in EXTI registers for STM32F04x, STM32F078xx and STM32F098xx devices. I2C updates Added IS_I2C_WAKEUP_FROMSTOP_INSTANCE definition for I2C instances supporting Wakeup from Stop mode. I2S updates Removed SPI_I2S prescaler register not supported by STM32F030x6 and STM32F030x8 devices. RCC updates Added missing RCC_CFGR_PLLNODIV definition for STM32F030x4/6 devices. RTC updates Removed cast from RTC_BKP_NUMBER definition. SYSCFG updates Renamed SYSCFG_CFGR1_IRDA_ENV_SEL bit definitions to SYSCFG_CFGR1_IR_MOD for SYSCFG_CFGR1 register. TIM updates Added IS_TIM_HALL_SENSOR_INTERFACE_INSTANCE definition. Added IS_TIM_ETR_INSTANCE definition. UART updates Renamed IS_UART_WAKEUP_INSTANCE to IS_UART_WAKEUP_FROMSTOP_INSTANCE. USART updates Defined USART_ISR_RWU bit for all STM32F0xx devices. ### V2.2.3 / 29-January-2016 Main Changes Added mention to STM32F091xB mcus missing in the list of mcus of stm32f0xx.h. Updated CMSIS Device compliancy with MISRA C 2004 rule 10.6. Updated CMSIS Device compliancy with MISRA C 2004 rule 5.1. Added HSI48_VALUE definition in system_stm32f0xx.c file. Put variable AHBPrescTable as external in system_stm32f0xx.h. Added channel selection bit definitions for for DMA1_CSELR register. Used RCC_CFGR_MCOSEL as reference in all the families. Renamed RCC_CFGR_MCOSEL_PLL to RCC_CFGR_MCOSEL_PLL_DIV2 for alignment between all families. Updated EWUPx pins defintions for STM32F042x6 and STM32F048xx devices. Added FLASHSIZE_BASE and UID_BASE defines. Added missing bits definition for RTC_TAFCR register. Added missing bits definition for I2C_OAR2 register (I2C_OAR2 mask values). Renamed I2C_CR1_DFN to I2C_CR1_DNF bit definition for I2C_CR1 register. Removed __IO or __I on constant table declaration. Used default DAC instance naming DAC1 in macro IS_DAC_ALL_INSTANCE(). Aligned EXTI registers Bits naming between all families. Aligned WWDG registers Bits naming between all families. Aligned COMP common instance definition. Corrected CRC defines: Replaced POL field by RESERVED3 for STM32F030x6, STM32F030x8, STM32F031x6, STM32F038xx, STM32F042x6, STM32F048xx devices. Corrected CRC defines: Removed Bit definitions related to Polynomial in CRC_CR and CRC_POL registers for STM32F030xC. Updated for ADC: removed conditions on CCR_TS definition. Corrected SYSCFG_RTC_WAKEUP and SYSCFG_RTC_ALRA Bits definition for SYSCFG_xxx ISR Wrapper register. Added ADC_CHSELR_CHSEL Bit definition for ADC_CHSELR register. Removed RCC_CSR_V18PWRRSTF Bit definition for STM32F0x8xx devices. Corrected USART defines for STM32F030xx, STM32F070xx devices. Removed IS_UART_AUTOBAUDRATE_DETECTION_INSTANCE macro definition. Adapted IS_USART_AUTOBAUDRATE_DETECTION_INSTANCE to device feature support. Removed IS_UART_DRIVER_ENABLE_INSTANCE definition for STM32F030x8, STM32F030xC and STM32F070xB devices. Corrected FLASH_OBR_nBOOT0 value. Removed Synchronous mode support on USART5/6 for STM32F030xC. Removed HW Flow Control support on USART5/6/7/8 for STM32F091xC. ### V2.2.2 / 26-June-2015 Main Changes Add missing WUT bits in EXTI_IMR/EMR/RTSR/FTSR/PR/SWIER for different IT lines. Add preprocessor compilation switch #define STM32F0 in stm32f0xx.h. Correct FLASH_KEY name difference between STM32F0 and STM32F3. Remove RCC_CFGR3_USART2SW from CMSIS, present only for STM32F07x and STM32F09x. Modify EXTI/COMP defines from uint16 to uint32. Add missing definitions of EXTI_IMR_MR31 used by PWREx in stm32f042x6 and stm32f048xx files. Add FLASH_BANK1_END defines. Remove WRP defines for few defines under devices swicthes. Add FLASH_OBR_RAM_PARITY_CHECK and FLASH_OBR_BOOT_SEL CMSIS files. ### V2.2.1 / 09-January-2015 Main Changes system_stm32f0xx.c: replace wrong compilation switch STM32F078xB by STM32F078xx. stm32F070xb.h: correct wrong DMA remap mask value for STM32f070xB. stm32F070xb.h, stm32F070x6.h, stm32F030xc.h: add missing macro IS_UART_DRIVER_ENABLE_INSTANCE() stm32F070xb.h, stm32F030xc.h: add missing RTC periodic Wakeup register & bits description ### V2.2.0 / 05-December-2014 Main Changes Add CMSIS files for new STM32F0 value line devices: STM32F030xC and STM32F070x6/xB. Add macro to check AF capability of gpio instance uint32_t alignement done on all Peripheral registers structures & bits definition stm32f091xc.h: DMA channel remap register renamed for compatibility with other STM32 devices startup_stm32f042x6.s & startup_stm32f070x6.s: fix boot issue ### V2.1.0 / 03-October-2014 Main Changes Add new CMSIS files for STM32F091xc and STM32F098xx products VDDIO2 IRQ missing in F07xx/F09xx/F04xx product IS_DAC_CHANNEL_INSTANCE macro removed as unused uint32_t partial alignement done on peripheral Bit definition & register structure Bit definition name error for DMA_RMPCR1 register of STM32F091xC Remove PDV feature on REGoff part Remove POSITION_VAL macro as it uses RBIT, CLZ instructions, that are not supported by Cortex-M0 GPIOS BSRR regsiter should not be split in BSRRH/BSRRL ### V2.0.1 / 18-June-2014 Main Changes General Add new macros IS_GPIO_LOCK_INSTANCE to check GPIO port with lock capability IS_UART_HALFDUPLEX_INSTANCE, IS_UART_LIN_INSTANCE and IS_UART_WAKEUP_INSTANCE to check the UART instance supported features. STM32F042x8 and STM32F048xx update Rename DMA1_Channel4_5_6_7_IRQn to DMA1_Channel4_5_IRQn Rename ADC1_COMP_IRQn to ADC1_IRQn Remove SPI2 instance STM32F051x8, STM32F058xx, STM32F071xB, STM32F072xB and STM32F078xx update Fix COMP2 instance base address Add new macro IS_COMP_DAC1SWITCH_INSTANCE to check COMP instance with switch of DAC1 channel1 output to non inverting input STM32F051x8 and STM32F058xx update Rename DMA1_Channel4_5_6_7_IRQn to DMA1_Channel4_5_IRQn STM32F078xx update Remove CAN peripheral description ### V2.0.0 / 28-May-2014 Main Changes Major update based on STM32Cube specification: new CMSIS device files release dedicated to STM32F030x4/x6, STM32F030x8, STM32F031x4/x6, STM32F051x4/x6/x8, STM32F071x8/xB, STM32F042x4/x6, STM32F072x8/xB, STM32F038xx, STM32F048xx, STM32F058xx and STM32F078xx devices. This version has to be used for STM32CubeF0 based development although files can be used independently too. ### V1.2.1 / 22-November-2013 Main Changes stm32f0xx.h Update STM32F030 devices definition: Remove the STM32F030X8 and STM32FO30X6 defines and replace them with the STM32F030 define Update IRQn enum for STM32F030 devices system_stm32f0xx.c SystemInit(): update to support STM32F030 devices Remove the startup files startup_stm32f030x8.s and startup_stm32f030x6.s and replace them by startup_stm32f030.s, for EWARM, MDK-ARM and Truestudio supported compilers ### V1.2.0 / 01-August-2013 Main Changes Add support of STM32F030 devices (STM32F030x8 and STM32F030x6 microcontrollers where the Flash memory ranges between 16 and 32 Kbytes) stm32f0xx.h Update STM32F0xx devices definition: Add new definition STM32F030X8 and STM32FO30X6 for STM32F030 devices Update IRQn enum for STM32F030 devices system_stm32f0xx.c SystemInit(): update to support STM32F030 devices Add new startup files, startup_stm32f030x8.s and startup_stm32f030x6.s, for EWARM, MDK-ARM and Truestudio supported compilers ### V1.1.1 / 31-July-2013 Main Changes stm32f0xx.h Extend HSE_STARTUP_TIMEOUT and HSI_STARTUP_TIMEOUT values to 0x5000 ### V1.1.0 / 10-May-2013 Main Changes Add support of STM32F0xx Low-density devices (STM32F050xx and STM32F060xx microcontrollers where the Flash memory ranges between 16 and 32 Kbytes) stm32f0xx.h Update STM32F0xx devices definition: Define for STM32F0xx Medium-density devices changed from STM32F0XX to STM32F0XX_MD Add new definition STM32F0XX_LD for STM32F0xx Low-density devices Update IRQn enum for STM32F0XX_LD devices Add new bits definition RCC_CFGR register: MCOPRE[0:2] and PLLNODIV SYSCFG_CFGR1 register: FMP_I2C1, FMP_PA9 and FMP_PA10 system_stm32f0xx.c SystemInit(): update to reset new bits added in RCC_CFGR register Add new startup files, startup_stm32f0xx_ld.s, for the supported compilers ### V1.0.2 / 13-July-2012 Main Changes stm32f0xx.h Fix issue with gcc_ride7 startup file ### V1.0.1 / 20-April-2012 Main Changes stm32f0xx.h Add reference to STM32F050xx (Flash memory up to 32 Kbytes) and STM32F051xx (Flash memory up to 64 Kbytes) devices RTC register bits definition: remove reference to Tamper3 ### V1.0.0 / 04-September-2012 Main Changes First official release for STM32F30x devices (Standard Library) ## License Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met: Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution. Neither the name of STMicroelectronics nor the names of its contributors may be used to endorse or promote products derived from this software without specific prior written permission. THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE. For complete documentation on STM32 Microcontrollers visit www.st.com/STM32