/**
  @page I2C_TwoBoards_ComIT I2C Two Boards Communication IT Example
  
  @verbatim
  ******************** (C) COPYRIGHT 2016 STMicroelectronics *******************
  * @file    I2C/I2C_TwoBoards_ComIT/readme.txt 
  * @author  MCD Application Team
  * @brief   Description of the I2C Two Boards Communication IT example.
  ******************************************************************************
  *
  * Redistribution and use in source and binary forms, with or without modification,
  * are permitted provided that the following conditions are met:
  *   1. Redistributions of source code must retain the above copyright notice,
  *      this list of conditions and the following disclaimer.
  *   2. Redistributions in binary form must reproduce the above copyright notice,
  *      this list of conditions and the following disclaimer in the documentation
  *      and/or other materials provided with the distribution.
  *   3. Neither the name of STMicroelectronics nor the names of its contributors
  *      may be used to endorse or promote products derived from this software
  *      without specific prior written permission.
  *
  * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
  * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
  * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
  * DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE
  * FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
  * DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
  * SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
  * CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY,
  * OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
  * OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
  @endverbatim

@par Example Description 

This example describes how to perform I2C data buffer transmission/reception between 
two boards using an interrupt.

Board: STM32F0308-Discovery RevA (embeds a STM32F030R8T6 device)
SCL Pin: PB6 (P2)
SDA Pin: PB7 (P2)

   _________________________                       _________________________ 
  |           ______________|                     |______________           |
  |          |I2C1          |                     |          I2C1|          |
  |          |              |                     |              |          |
  |          |          SCL |_____________________| SCL          |          |
  |          |              |                     |              |          |
  |          |              |                     |              |          |
  |          |              |                     |              |          |
  |          |          SDA |_____________________| SDA          |          |
  |          |              |                     |              |          |
  |          |______________|                     |______________|          |
  |                         |                     |                         |
  |                      GND|_____________________|GND                      |
  |_STM32_Board 1___________|                     |_STM32_Board 2___________|

At the beginning of the main program the HAL_Init() function is called to reset 
all the peripherals, initialize the Flash interface and the systick.
Then the SystemClock_Config() function is used to configure the system
clock (SYSCLK) to run at 48 MHz.

The I2C peripheral configuration is ensured by the HAL_I2C_Init() function.
This later is calling the HAL_I2C_MspInit()function which core is implementing
the configuration of the needed I2C resources according to the used hardware (CLOCK, 
GPIO and NVIC). You may update this function to change I2C configuration.

The I2C communication is then initiated.
The project is split in two parts: the Master Board and the Slave Board
- Master Board
  The HAL_I2C_Master_Receive_IT() and the HAL_I2C_Master_Transmit_IT() functions 
  allow respectively the reception and the transmission of a predefined data buffer
  in Master mode using interrupt.
- Slave Board
  The HAL_I2C_Slave_Receive_IT() and the HAL_I2C_Slave_Transmit_IT() functions 
  allow respectively the reception and the transmission of a predefined data buffer
  in Slave mode using interrupt.
The user can choose between Master and Slave through "#define MASTER_BOARD"
in the "main.c" file:
- Uncomment "#define MASTER_BOARD" to select Master board.
- Comment "#define MASTER_BOARD" to select Slave board.

For this example the aTxBuffer is predefined and the aRxBuffer size is same as aTxBuffer.

In a first step after the user press the User push-button on the Master Board,
I2C Master starts the communication by sending aTxBuffer through HAL_I2C_Master_Transmit_IT()
to I2C Slave which receives aRxBuffer through HAL_I2C_Slave_Receive_IT(). 
The second step starts when the user press the User push-button on the Master Board,
the I2C Slave sends aTxBuffer through HAL_I2C_Slave_Transmit_IT()
to the I2C Master which receives aRxBuffer through HAL_I2C_Master_Receive_IT().
The end of this two steps are monitored through the HAL_I2C_GetState() function
result.
Finally, aTxBuffer and aRxBuffer are compared through Buffercmp() in order to 
check buffers correctness.  

STM32F0308-Discovery RevA's LEDs can be used to monitor the transfer status:
 - LED3 is ON when the transmission process is complete.
 - LED3 is OFF when the reception process is complete.
 - LED4 is ON when there is an error in transmission/reception process.  

@note I2Cx instance used and associated resources can be updated in "main.h"
file depending hardware configuration used.

@note Care must be taken when using HAL_Delay(), this function provides accurate delay (in milliseconds)
      based on variable incremented in SysTick ISR. This implies that if HAL_Delay() is called from
      a peripheral ISR process, then the SysTick interrupt must have higher priority (numerically lower)
      than the peripheral interrupt. Otherwise the caller ISR process will be blocked.
      To change the SysTick interrupt priority you have to use HAL_NVIC_SetPriority() function.

@note The application need to ensure that the SysTick time base is always set to 1 millisecond
      to have correct HAL operation.

@par Directory contents 

  - I2C/I2C_TwoBoards_ComIT/Inc/stm32f0xx_hal_conf.h    HAL configuration file
  - I2C/I2C_TwoBoards_ComIT/Inc/stm32f0xx_it.h          I2C interrupt handlers header file
  - I2C/I2C_TwoBoards_ComIT/Inc/main.h                  Header for main.c module  
  - I2C/I2C_TwoBoards_ComIT/Src/stm32f0xx_it.c          I2C interrupt handlers
  - I2C/I2C_TwoBoards_ComIT/Src/main.c                  Main program
  - I2C/I2C_TwoBoards_ComIT/Src/system_stm32f0xx.c      STM32F0xx system source file
  - I2C/I2C_TwoBoards_ComIT/Src/stm32f0xx_hal_msp.c     HAL MSP file    


@par Hardware and Software environment

  - This example runs on STM32F030R8 devices.
    
  - This example has been tested with STM32F0308-Discovery RevA board and can be
    easily tailored to any other supported device and development board.    

  - STM32F0308-Discovery RevA Set-up
    - Connect I2C_SCL line of Master board (PB6, P2) to I2C_SCL line of Slave Board (PB6, P2).
    - Connect I2C_SDA line of Master board (PB7, P2) to I2C_SDA line of Slave Board (PB7, P2).
    - Connect GND of Master board to GND of Slave Board.

@par How to use it ? 

In order to make the program work, you must do the following :
 - Open your preferred toolchain 
 - Rebuild all files and load your image into target memory
    o Uncomment "#define MASTER_BOARD" and load the project in Master Board
    o Comment "#define MASTER_BOARD" and load the project in Slave Board
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
