/**
  @page DFU_Standalone USB Device Firmware Upgrade (DFU) Example
  
  @verbatim
  ******************** (C) COPYRIGHT 2016 STMicroelectronics *******************
  * @file    USB_Device/DFU_Standalone/readme.txt 
  * @author  MCD Application Team
  * @version V1.6.0
  * @date    12-May-2017
  * @brief   Description of the USB DFU example.
  ******************************************************************************
  * @attention
  *
  * <h2><center>&copy; Copyright © 2016 STMicroelectronics International N.V. 
  * All rights reserved.</center></h2>
  *
  * Redistribution and use in source and binary forms, with or without 
  * modification, are permitted, provided that the following conditions are met:
  *
  * 1. Redistribution of source code must retain the above copyright notice, 
  *    this list of conditions and the following disclaimer.
  * 2. Redistributions in binary form must reproduce the above copyright notice,
  *    this list of conditions and the following disclaimer in the documentation
  *    and/or other materials provided with the distribution.
  * 3. Neither the name of STMicroelectronics nor the names of other 
  *    contributors to this software may be used to endorse or promote products 
  *    derived from this software without specific written permission.
  * 4. This software, including modifications and/or derivative works of this 
  *    software, must execute solely and exclusively on microcontroller or
  *    microprocessor devices manufactured by or for STMicroelectronics.
  * 5. Redistribution and use of this software other than as permitted under 
  *    this license is void and will automatically terminate your rights under 
  *    this license. 
  *
  * THIS SOFTWARE IS PROVIDED BY STMICROELECTRONICS AND CONTRIBUTORS "AS IS" 
  * AND ANY EXPRESS, IMPLIED OR STATUTORY WARRANTIES, INCLUDING, BUT NOT 
  * LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY, FITNESS FOR A 
  * PARTICULAR PURPOSE AND NON-INFRINGEMENT OF THIRD PARTY INTELLECTUAL PROPERTY
  * RIGHTS ARE DISCLAIMED TO THE FULLEST EXTENT PERMITTED BY LAW. IN NO EVENT 
  * SHALL STMICROELECTRONICS OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
  * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
  * LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, 
  * OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF 
  * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING 
  * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE,
  * EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
  @endverbatim

@par Example Description 

This application presents a compliant implementation of the Device Firmware Upgrade (DFU) 
capability for programming the embedded flash memory through the USB peripheral.

This is a typical example on how to use the STM32F1xx USB Device peripheral to implement the DFU
capability for programming the embedded flash memory of the STM32F1xx devices.

At the beginning of the main program the HAL_Init() function is called to reset all the peripherals,
initialize the Flash interface and the systick. The user is provided with the SystemClock_Config()
function to configure the system clock (SYSCLK) to run at 72 MHz. The Full Speed (FS) USB module uses
internally a 48-MHz clock, which is generated from an integrated PLL.

The DFU transactions are based on Endpoint 0 (control endpoint) transfer. All requests and status 
control are sent/received through this endpoint.

The Internal flash memory memory is split as follows:
 - DFU area located in [0x08000000 : USBD_DFU_APP_DEFAULT_ADD-1]: Only read access
 - Application area located in [USBD_DFU_APP_DEFAULT_ADD : Device's end address]: Read, Write, and Erase
   access

In this application, two operating modes are available:
 1. DFU operating mode: 
    This mode is entered after an MCU reset in case:
     - The DFU mode is forced by the user: the user presses the key button.
     - No valid code found in the application area: a code is considered valid if the MSB of the initial
       Main Stack Pointer (MSP) value located in the first address of the application area is equal to 
       0x2000
      
 2. Run-time application mode: 
    This is the normal run-time activities. A binary which toggles LEDs on the STM3210C-EVAL board is 
    provided in Binary directory.

@note After each device reset, hold down the Key push-button on the board to enter the DFU mode.     

Traditionally, firmware is stored in Hex, S19 or Binary files, but these formats do not contain the 
necessary information to perform the upgrade operation, they contain only the actual data of the program
to be downloaded. However, the DFU operation requires more information, such as the product identifier, 
vendor identifier, Firmware version and the Alternate setting number (Target ID) of the target to be 
used, this information makes the upgrade targeted and more secure. To add this information, DFU file 
format is used. For more details refer to the "DfuSe File Format Specification" document (UM0391).

To generate a DFU image, download "DFUse Demonstration" tool and use DFU File Manager to convert a 
binary image into a DFU image. This tool is for download from www.st.com
To download a *.dfu image, use "DfuSe Demo" available within "DFUse Demonstration" install directory. 

Please refer to UM0412, DFuSe USB device firmware upgrade STMicroelectronics extension for more details
on the driver installation and PC host user interface.

@note The application needs to ensure that the SysTick time base is set to 1 millisecond
      to have correct HAL configuration.

@note Care must be taken when using HAL_Delay(), this function provides accurate delay (in milliseconds)
      based on variable incremented in SysTick ISR. This implies that if HAL_Delay() is called from
      a peripheral ISR process, then the SysTick interrupt must have higher priority (numerically lower)
      than the peripheral interrupt. Otherwise the caller ISR process will be blocked.
      To change the SysTick interrupt priority you have to use HAL_NVIC_SetPriority() function.

For more details about the STM32Cube USB Device library, please refer to UM1734 
"STM32Cube USB Device library".
      

@par USB Library Configuration

It is possible to fine tune needed USB Device features by modifying defines values in USBD configuration
file “usbd_conf.h” available under the project includes directory, in a way to fit the application
requirements, such as:      
 - USBD_DFU_APP_DEFAULT_ADD, specifying the address from where user's application will be downloaded.

Device's end address is the end address of the flash memory and it is dependent on the device in use.

@par Directory contents 

  - USB_Device/DFU_Standalone/Inc/stm32f1xx_hal_conf.h    HAL configuration file
  - USB_Device/DFU_Standalone/Inc/stm32f1xx_it.h          IT interrupt handlers header file
  - USB_Device/DFU_Standalone/Inc/main.h                  Main program header file
  - USB_Device/DFU_Standalone/Inc/usbd_dfu_flash.h        Internal flash memory management header file
  - USB_Device/DFU_Standalone/Inc/usbd_conf.h             USB device driver Configuration file
  - USB_Device/DFU_Standalone/Inc/usbd_desc.h             USB device descriptor header file
  - USB_Device/DFU_Standalone/Src/stm32f1xx_it.c          IT interrupt handlers
  - USB_Device/DFU_Standalone/Src/main.c                  Main program
  - USB_Device/DFU_Standalone/Src/usbd_conf.c             USB Device library callbacks and MSP
  - USB_Device/DFU_Standalone/Src/usbd_dfu_flash.c        Internal flash memory management
  - USB_Device/DFU_Standalone/Src/usbd_desc.c             USBD descriptors and string formatting method
  - USB_Device/DFU_Standalone/Src/system_stm32f1xx.c      STM32F1xx system source file

@par Hardware and Software environment

  - This example runs on STM32F107x devices.
    
  - This example has been tested with a STM3210C-EVAL board embedding
    a STM32F107x device and can be easily tailored to any other supported device
    and development board.

  - STM3210C-EVAL Set-up
    - Connect the STM3210C-EVAL board to the PC through 'USB Type micro A-Male
      to A-Male' cable.

@par How to use it ?

In order to make the program work, you must do the following :
 - Open your preferred toolchain
 - Rebuild all files and load your image into target memory
 - To run the example, proceed as follows:
   - Install "DfuSe Demonstrator"
   - Install the DFU driver available in "DfuSe Demonstrator" installation directory 
   - Open "DfuSe Demo" and download the "STM3210C-EVAL_SysTick_0x08005000.dfu"
     provided in Binary directory.
   - To run the downloaded application, execute the command "leave the DFU mode"
     or simply reset the board.

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
