/**
  @page TIM_DMA TIM example
  
  @verbatim
  ******************** (C) COPYRIGHT 2016 STMicroelectronics *******************
  * @file    Examples_LL/TIM/TIM_DMA/readme.txt 
  * @author  MCD Application Team
  * @version V1.0.0
  * @date    14-April-2017
  * @brief   Description of the TIM_DMA example.
  ******************************************************************************
  *
  * Redistribution and use in source and binary forms, with or without modification,
  * are permitted provided that the following conditions are met:
  *   1. Redistributions of source code must retain the above copyright notice,
  *      this list of conditions and the following disclaimer.
  *   2. Redistributions in binary form must reproduce the above copyright notice,
  *      this list of conditions and the following disclaimer in the documentation
  *      and/or other materials provided with the distribution.
  *   3. Neither the name of STMicroelectronics nor the names of its contributors
  *      may be used to endorse or promote products derived from this software
  *      without specific prior written permission.
  *
  * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
  * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
  * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
  * DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE
  * FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
  * DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
  * SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
  * CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY,
  * OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
  * OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
  @endverbatim

@par Example Description

This example provides a description of how to use DMA
with timer update request to transfer data from memory to
TIMER Capture Compare Register 3 (TIMx_CCR3). This
example uses the STM32F1xx TIM LL API. The
peripheral initialization is done using LL unitary services
functions for optimization purpose (performance and size).

The following configuration values are used in this example:
  - TIM3CLK = SystemClock
  - Counter repetition = 3 
  - Prescaler = 0 
  - TIM3 counter clock = SystemClock
  - SystemCoreClock is set to 72 MHz for STM32F1xx Devices.

The objective is to configure TIM3 channel 3 to generate PWM edge aligned 
signal with a frequency equal to 17.57 KHz, and a variable duty cycle that
is changed by the DMA after a specific number of Update DMA request.

The number of this repetitive requests is defined by the TIM3 Repetition counter,
each 4 Update Requests, the TIM3 Channel 3 Duty Cycle changes to the next new 
value defined by the aCCValue_Buffer.

The PWM waveform can be displayed using an oscilloscope.

Whenever a DMA transfer fails LED2 flashes with a frequency of 1 Hz.
 
@note PWM signal frequency value mentioned above is theoretical (obtained when
      the system clock frequency is exactly 80 MHz). Since the generated system
      clock frequency may vary from one board to another observed PWM signal
      frequency might be slightly different.

@par Directory contents 

  - TIM/TIM_DMA/Inc/stm32f1xx_it.h          Interrupt handlers header file
  - TIM/TIM_DMA/Inc/main.h                  Header for main.c module
  - TIM/TIM_DMA/Inc/stm32_assert.h          Template file to include assert_failed function
  - TIM/TIM_DMA/Src/stm32f1xx_it.c          Interrupt handlers
  - TIM/TIM_DMA/Src/main.c                  Main program
  - TIM/TIM_DMA/Src/system_stm32f1xx.c      STM32F1xx system source file


@par Hardware and Software environment

  - This example runs on STM32F103xB devices.
    
  - This example has been tested with STM32F103RB-Nucleo board and can be
    easily tailored to any other supported device and development board.

  - STM32F103RB-Nucleo Set-up
    - Connect TIM3 pin to the oscilloscope to monitor the generated waveform:
      - TIM3_CH3  PB.00: connected to pin 4 of CN8 connector 

@par How to use it ? 

In order to make the program work, you must do the following :
 - Open your preferred toolchain
 - Rebuild all files and load your image into target memory
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
