/**
  @page ADC_MultiChannelSingleConversion ADC example
  
  @verbatim
  ******************** (C) COPYRIGHT 2017 STMicroelectronics *******************
  * @file    Examples_LL/ADC/ADC_MultiChannelSingleConversion/readme.txt 
  * @author  MCD Application Team
  * @brief   Description of the ADC_MultiChannelSingleConversion example.
  ******************************************************************************
  *
  * Redistribution and use in source and binary forms, with or without modification,
  * are permitted provided that the following conditions are met:
  *   1. Redistributions of source code must retain the above copyright notice,
  *      this list of conditions and the following disclaimer.
  *   2. Redistributions in binary form must reproduce the above copyright notice,
  *      this list of conditions and the following disclaimer in the documentation
  *      and/or other materials provided with the distribution.
  *   3. Neither the name of STMicroelectronics nor the names of its contributors
  *      may be used to endorse or promote products derived from this software
  *      without specific prior written permission.
  *
  * THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS"
  * AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE
  * IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE
  * DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT HOLDER OR CONTRIBUTORS BE LIABLE
  * FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL
  * DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR
  * SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER
  * CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY,
  * OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE
  * OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
  @endverbatim

@par Example Description
This example describes how to use a ADC peripheral to convert several channels, 
ADC conversions are performed successively in a scan sequence; 
This example is based on the STM32F2xx ADC LL API; 
peripheral initialization done using LL unitary services functions
for optimization purpose (performance and size).

Example configuration:
ADC is configured in single conversion mode, from SW trigger.
Sequencer of group regular (default group available on ADC of all STM32 devices)
is configured to convert 3 channels: 1 channel from GPIO, 2 internal channels:
temperature sensor and VrefInt.
DMA is configured to transfer conversion data in an array of size three (one array
address for conversion data of each channel), in circular mode to update
results array at each ADC sequence conversions.

Example execution:
At each press on User Button, the ADC executes the scan sequence: 
ADC performs conversion of the three selected channels successively,
in burst (discontinuous mode not enabled).
The 3 ADC conversions data are transferred by DMA into the results array
"aADCxConvertedData".
ADC conversion data of each sequence rank is at an address of the array:
 - aADCxConvertedData[0]: ADC channel set on rank1 (GPIO as analog input)
 - aADCxConvertedData[1]: ADC channel set on rank2 (VrefInt)
 - aADCxConvertedData[2]: ADC channel set on rank3 (Temperature sensor)
LED1 is turned on when ADC conversions and DMA transfer of the sequence
are completed.

ADC conversions raw data are computed to physical values
using LL ADC driver helper macro:
 - Value of voltage on GPIO pin (on which is mapped ADC channel) (unit: mV)
 - Value of internal voltage reference VrefInt (unit: mV)
 - Value of temperature (unit: degree Celcius)

For debug: variables to monitor with debugger watch window:
 - "aADCxConvertedData": ADC group regular conversion data
 - "ubDmaTransferStatus": status of DMA transfer of ADC group regular conversions
 - "uhADCxConvertedData_VoltageGPIO_mVolt":        Value of voltage on GPIO pin (on which is mapped ADC channel) (unit: mV)
 - "uhADCxConvertedData_VrefInt_mVolt":            Value of internal voltage reference VrefInt (unit: mV)
 - "hADCxConvertedData_Temperature_DegreeCelsius": Value of temperature (unit: degree Celcius)

Connection needed:
Use an external power supply, adjust supply voltage and connect it to analog input pin (cf pin below).

Other peripherals used:
  1 GPIO for User Button
  1 GPIO for LED1
  1 GPIO for analog input: PA.04 ( connector CN7 pin 17)
  DMA

@par Directory contents 

  - ADC/ADC_MultiChannelSingleConversion/Inc/stm32f2xx_it.h          Interrupt handlers header file
  - ADC/ADC_MultiChannelSingleConversion/Inc/main.h                  Header for main.c module
  - ADC/ADC_MultiChannelSingleConversion/Inc/stm32_assert.h          Template file to include assert_failed function
  - ADC/ADC_MultiChannelSingleConversion/Src/stm32f2xx_it.c          Interrupt handlers
  - ADC/ADC_MultiChannelSingleConversion/Src/main.c                  Main program
  - ADC/ADC_MultiChannelSingleConversion/Src/system_stm32f2xx.c      STM32F2xx system source file


@par Hardware and Software environment

  - This example runs on STM32F207xx devices.
    
  - This example has been tested with NUCLEO-F207ZG board and can be
    easily tailored to any other supported device and development board.


@par How to use it ? 

In order to make the program work, you must do the following :
 - Open your preferred toolchain
 - Rebuild all files and load your image into target memory
 - Run the example

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
