/**
  @page LibJPEG_Encoding LibJPEG encoding application
  
  @verbatim
  ******************** (C) COPYRIGHT 2017 STMicroelectronics *******************
  * @file    LibJPEG/LibJPEG_Encoding/Readme.txt 
  * @author  MCD Application Team
  * @brief   Description of the LibJPEG encoding application.
  ******************************************************************************
  * @attention
  *
  * <h2><center>&copy; Copyright © 2017 STMicroelectronics International N.V. 
  * All rights reserved.</center></h2>
  *
  * Redistribution and use in source and binary forms, with or without 
  * modification, are permitted, provided that the following conditions are met:
  *
  * 1. Redistribution of source code must retain the above copyright notice, 
  *    this list of conditions and the following disclaimer.
  * 2. Redistributions in binary form must reproduce the above copyright notice,
  *    this list of conditions and the following disclaimer in the documentation
  *    and/or other materials provided with the distribution.
  * 3. Neither the name of STMicroelectronics nor the names of other 
  *    contributors to this software may be used to endorse or promote products 
  *    derived from this software without specific written permission.
  * 4. This software, including modifications and/or derivative works of this 
  *    software, must execute solely and exclusively on microcontroller or
  *    microprocessor devices manufactured by or for STMicroelectronics.
  * 5. Redistribution and use of this software other than as permitted under 
  *    this license is void and will automatically terminate your rights under 
  *    this license. 
  *
  * THIS SOFTWARE IS PROVIDED BY STMICROELECTRONICS AND CONTRIBUTORS "AS IS" 
  * AND ANY EXPRESS, IMPLIED OR STATUTORY WARRANTIES, INCLUDING, BUT NOT 
  * LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY, FITNESS FOR A 
  * PARTICULAR PURPOSE AND NON-INFRINGEMENT OF THIRD PARTY INTELLECTUAL PROPERTY
  * RIGHTS ARE DISCLAIMED TO THE FULLEST EXTENT PERMITTED BY LAW. IN NO EVENT 
  * SHALL STMICROELECTRONICS OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
  * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
  * LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, 
  * OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF 
  * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING 
  * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE,
  * EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
   @endverbatim

@par Application Description

This application demonstrates how to read BMP file from micro SD, encode it, save the jpeg file
in uSD Card then decode the jpeg file and display the final BMP image on the LCD.

BMP image is read from the bottom to the top, in order to be encoded in JPG from the top to the bottom.
BMP image is in BGR format and JPG in RGB format. B and R values of the pixels are swapped by redefining
the order of pixel components.

The BMP image should be copied at the micro SD card root.The .bmp 
files available within the "BMP_320x240" folder under "Utilities/Media/Pictures"

The images must have the following properties:
 - named as "image.bmp"
 - 320*240 size

The image size can be modified by changing IMAGE_WIDTH and IMAGE_HEIGHT defines 
in "main.h" file to decode other resolution than 320x240.    

@note Care must be taken when using HAL_Delay(), this function provides accurate delay (in milliseconds)
      based on variable incremented in SysTick ISR. This implies that if HAL_Delay() is called from
      a peripheral ISR process, then the SysTick interrupt must have higher priority (numerically lower)
      than the peripheral interrupt. Otherwise the caller ISR process will be blocked.
      To change the SysTick interrupt priority you have to use HAL_NVIC_SetPriority() function.
      
@note The application needs to ensure that the SysTick time base is always set to 1 millisecond
      to have correct HAL operation.


@par Directory contents

    - LibJPEG/LibJPEG_Encoding/Inc/main.h                      Main program header file
    - LibJPEG/LibJPEG_Encoding/Inc/stm32f2xx_it.h              Interrupt handlers header file
    - LibJPEG/LibJPEG_Encoding/Inc/stm32f2xx_hal_conf.h        HAL Configuration file 
    - LibJPEG/LibJPEG_Encoding/Inc/ffconf.h                    FAT file system module configuration file
    - LibJPEG/LibJPEG_Encoding/Inc/encode.h                    Encoder header file
    - LibJPEG/LibJPEG_Encoding/Inc/decode.h                    Decoder header file
    - LibJPEG/LibJPEG_Encoding/Inc/jmorecfg.h                  Lib JPEG configuration file (advanced configuration).
    - LibJPEG/LibJPEG_Encoding/Inc/jconfig.h                   Lib JPEG configuration file.
    - LibJPEG/LibJPEG_Decoding/Inc/jdata_conf.h                Write/Read methods definition
    - LibJPEG/LibJPEG_Encoding/Src/main.c                      Main program  
    - LibJPEG/LibJPEG_Encoding/Src/stm32f2xx_it.c              Interrupt handlers
    - LibJPEG/LibJPEG_Encoding/Src/system_stm32f2xx.c          STM32F2xx system clock configuration file
    - LibJPEG/LibJPEG_Encoding/Src/encode.c                    Encoder file
    - LibJPEG/LibJPEG_Encoding/Src/decode.c                    Decoder file
    - LibJPEG/LibJPEG_Decoding/Src/jdata_conf.c                Write/Read methods definition



@par Hardware and Software environment

  - This application runs on STM32F207xx/217xx device.
    
  - This application has been tested with STMicroelectronics STM322xG-EVAL 
    evaluation boards and can be easily tailored to any other supported device 

  - STM322xG-EVAL Set-up
   - Connect a uSD Card to the MSD connector (CN6). 
   - Please ensure that jumpers JP16 and JP22 are in position 1-2.

@par How to use it ?

In order to make the program work, you must do the following :
 - Open your preferred toolchain 
 - Rebuild all files and load your image into target memory
 - Run the application

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
                                   
