/**
  @page Binary Description of the binary template
  
  @verbatim
  ******************** (C) COPYRIGHT 2017 STMicroelectronics *******************
  * @file    USB_Device/DFU_Standalone/Binary/Readme.txt 
  * @author  MCD Application Team
  * @brief   Description of the binary template application.
  ******************************************************************************
  * @attention
  *
  * <h2><center>&copy; Copyright © 2017 STMicroelectronics International N.V. 
  * All rights reserved.</center></h2>
  *
  * Redistribution and use in source and binary forms, with or without 
  * modification, are permitted, provided that the following conditions are met:
  *
  * 1. Redistribution of source code must retain the above copyright notice, 
  *    this list of conditions and the following disclaimer.
  * 2. Redistributions in binary form must reproduce the above copyright notice,
  *    this list of conditions and the following disclaimer in the documentation
  *    and/or other materials provided with the distribution.
  * 3. Neither the name of STMicroelectronics nor the names of other 
  *    contributors to this software may be used to endorse or promote products 
  *    derived from this software without specific written permission.
  * 4. This software, including modifications and/or derivative works of this 
  *    software, must execute solely and exclusively on microcontroller or
  *    microprocessor devices manufactured by or for STMicroelectronics.
  * 5. Redistribution and use of this software other than as permitted under 
  *    this license is void and will automatically terminate your rights under 
  *    this license. 
  *
  * THIS SOFTWARE IS PROVIDED BY STMICROELECTRONICS AND CONTRIBUTORS "AS IS" 
  * AND ANY EXPRESS, IMPLIED OR STATUTORY WARRANTIES, INCLUDING, BUT NOT 
  * LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY, FITNESS FOR A 
  * PARTICULAR PURPOSE AND NON-INFRINGEMENT OF THIRD PARTY INTELLECTUAL PROPERTY
  * RIGHTS ARE DISCLAIMED TO THE FULLEST EXTENT PERMITTED BY LAW. IN NO EVENT 
  * SHALL STMICROELECTRONICS OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
  * INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT
  * LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, 
  * OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF 
  * LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING 
  * NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE,
  * EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
  *
  ******************************************************************************
  @endverbatim

@par Application Description 

This directory contains a binary template (in DFU format) to be loaded into Flash memory using Device 
Firmware Upgrade application. This file was converted to the DFU format using the "DFU File Manager Tool"
included in the "DfuSe" PC software install.
For more details on how to convert a .bin file to DFU format please refer to the UM0412 user manual 
"Getting started with DfuSe USB device firmware upgrade STMicroelectronics extension" available from the
STMicroelectronics microcontroller website www.st.com.
   
This binary is a simple LED chaser. The 4 LEDs lights one by one for a period of 200 ms and the cycle 
repeats giving the running light appearance.
The system Timer (Systick) is used for to generate the delay.
The offset address of this binary is 0x0800C000 which matches the definition in DFU application
"USBD_DFU_APP_DEFAULT_ADD".


@par Hardware and Software environment

  - This application runs on STM32F207xx/STM32F217xx devices.
    
  - This application has been tested with STMicroelectronics STM322xG-EVAL 
    evaluation boards and can be easily tailored to any other supported device 
    and development board.  

 * <h3><center>&copy; COPYRIGHT STMicroelectronics</center></h3>
 */
