{"text_format":"2","workbook":"xls","n_sheets":3,"sheets":["Лист1","Лист2","Лист3"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Лист1","index":0,"n_rows":77,"n_cols":10,"rows_kept":77,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["Контакт","Сигнал","Наименование DEC","нумерация DEC","Описание","Наименование сигнала","Новое наименование",null,"анализатор"]
["А:А1","К ТПР5 Н","B IRQ5 L","AA1","Запрос прерывания",null,null,"?"]
["А:А2","К ТПР6 Н","B IRQ6 L","AB1","Запрос прерывания",null,null,"?"]
["А:А3","К А16 Н","B AD16 L","AC1","Адрес",null,"A16",null,"B10",28]
["А:А4","К А17 Н","B AD17","AD1","Адрес",null,"A17",null,"B11",30]
["А:А5","РЕЗ1","S SPARE1","AE1"]
["А:А6","РЕЗ2","S SPARE2","AF1"]
["А:А7","РЕЗ3","S SPARE3","AH1"]
["А:А8","ОБЩ","GND","AJ1","общий","GND","общий"]
["А:А9","ОТЛ1","M SPAREA","AK1"]
["А:А10","ОТЛ1","M SPAREA","AL1"]
["А:А11","ОБЩ","GND","AM1",null,"GND","общий"]
["А:А12","К ТПД Н","B DMR L","AN1","Требование прямого доступа (запрос к магистрали)",null,null,null,"B7",20]
["А:А13","К ОСТ Н","B HALT L","AP1","Останов","HALT","ОСТ",null,"B6",22]
["А:А14","К РГН Н","B REF L","AR1","Регенерация памяти","REF","РГН"]
["А:А15","ПРЕЗ1","PS PARE3","AS1"]
["А:А16","ОБЩ","GND","AT1"]
["А:А17","ПРЕЗ2","P SPARE3","AU1"]
["А:А18","+5ВБ","+5VB","AV1","питание","питание","питание"]
[]
["Б:А1","К ПОСТН В","B DCOK H","BA1","Постоянное напряжение нормальное (авария источника питания)","DCOK","АИП"]
["Б:А2","К ПИТН В","B POK H","BB1","Сетевое питание нормальное (авария сетевого питания)","POK","АСП"]
["Б:А3","К А18 Н","B DAL 18 L","BC1","Адрес",null,"A18",null,"B12",32]
["Б:А4","К А19 Н","B DAL 19 L","BD1","Адрес",null,"A19",null,"B13",34]
["Б:А5","К А20 Н","B DAL 20 L","BE1","Адрес",null,"A20",null,"B14",36]
["Б:А6","К А21 Н","B DAL 21 L","BF1","Адрес",null,"A21",null,"B15",38]
["Б:А7","Рез8","SPARE8","BH1"]
["Б:А8","Общ","GND","BJ1","общий","GND","общий"]
["Б:А9","ОТЛ2","M SPAREB","BK1"]
["Б:А10","ОТЛ2","M SPAREB","BL1"]
["Б:А11","Общ","GND","BM1","общий","GND","общий"]
["Б:А12","К ПВ Н","B SACK L","BN1","Подтверждение выборки(запроса) системного канала(магистрали)","SACK","ПЗ",null,"B8",24]
["Б:А13","К ТПР7 Н","B IRQ7 L","BP1","Запрос прерывания",null,null,"?"]
["Б:А14","К ПРТ Н","B EVNT L","BR1","Прерывание по таймеру (внешнему событию)","EVNT","ПВС"]
["Б:А15","ПРЕЗ3","P SPARE4","BS1"]
["Б:А16","Общ","GND","BT1","общий","GND","общий"]
["Б:А17","През4","P SPARE2","BU1"]
["Б:А18","+5В","+5V","BV1","питание","питание","питание"]
[]
["А:Б1","+5В","+5V","AA2","питание","питание","питание"]
["А:Б2","-12В","-12V","AB2","питание","питание","питание"]
["А:Б3","Общ","GND","AC2","общий","GND","общий"]
["А:Б4","+12В","+12V","AD2","питание","питание","питание"]
["А:Б5","К ВЫВОД Н","B DOUT L","AE2","Вывод(запись) данных","DOUT","ДЗП",null,"B0",8]
["А:Б6","К СИП Н","B RPLY L","AF2","Ответ пассивного устройства","RPLY","ОТВ",null,"B1",10]
["А:Б7","К ВВОД Н","B DIN L","AH2","Ввод(чтение) данных","DIN","ДЧТ",null,"B2",12]
["А:Б8","К СИА Н","B SYNC L","AJ2","Синхронизация активного устройства","SYNC","ОБМ",null,"B3",14]
["А:Б9","К Байт Н","B WTBT L","AK2","Выбор (признак записи) байта","WTBT","ПЗП",null,"B4",16]
["А:Б10","К ТПР4 Н","B IRQ 4 L","AL2","Запрос прерывания",null,null,"?"]
["А:Б11","К ППРI Н","B IAKI L","AM2","Предоставление (разрещение) прерываний (вход)","IAKI","ПРРI","?"]
["А:Б12","К ППРO Н","B IAKO L","AN2","Предоставление (разрещение) прерываний (выход)","IAKO","ПРРO","?"]
["А:Б13","К ВУ Н","B BS7 L","AP2","Выбор внешних устройств","BS7","ВУ",null,"B5",18]
["А:Б14","К ППДI Н","B DMGI L","AR2","Предоставление прямого доступа (разрешение захвата магистрали) вход","DMGI","РЗМI","?"]
["А:Б15","К ППДO Н","B DMGO L","AS2","Предоставление прямого доступа (разрешение захвата магистрали) выход","DMGO","РЗМO","?"]
["А:Б16","К СБРОС Н","B INIT L","AT2","Начальная установка","INIT","УСТ",null,"B9",26]
["А:Б17","К ДА00 Н","B DAL0","AU2","Адрес-данные","DAL00","АД00",null,"A0",7]
["А:Б18","К ДА01 Н","B DAL1","AV2","Адрес-данные","DAL01","АД01",null,"A1",9]
[]
["Б:Б1","+5В","+5","BA2","питание","питание","питание"]
["Б:Б2","-12В","-12","BB2","питание","питание","питание"]
["Б:Б3","Общ","GND","BC2","общий","общий","общий",null,"GND","1,2,5,6"]
["Б:Б4","+12В","+12","BD2","питание","питание","питание"]
["Б:Б5","К ДА 02 Н","B DAL2","BE2","Адрес-данные","DAL02","АД02",null,"A2",11]
["Б:Б6","К ДА 03 Н","B DAL3","BF2","Адрес-данные","DAL03","АД03",null,"A3",13]
["Б:Б7","К ДА 04 Н","B DAL4","BH2","Адрес-данные","DAL04","АД04",null,"A4",15]
["Б:Б8","К ДА 05 Н","B DAL5","BJ2","Адрес-данные","DAL05","АД05",null,"A5",17]
["Б:Б9","К ДА 06 Н","B DAL6","BK2","Адрес-данные","DAL06","АД06",null,"A6",19]
["Б:Б10","К ДА 07 Н","B DAL7","BL2","Адрес-данные","DAL07","АД07",null,"A7",21]
["Б:Б11","К ДА 08 Н","B DAL8","BM2","Адрес-данные","DAL08","АД08",null,"A8",23]
["Б:Б12","К ДА 09 Н","B DAL9","BN2","Адрес-данные","DAL09","АД09",null,"A9",25]
["Б:Б13","К ДА 10 Н","B DAL10","BP2","Адрес-данные","DAL10","АД10",null,"A10",27]
["Б:Б14","К ДА 11 Н","B DAL11","BR2","Адрес-данные","DAL11","АД11",null,"A11",29]
["Б:Б15","К ДА 12 Н","B DAL12","BS2","Адрес-данные","DAL12","АД12",null,"A12",31]
["Б:Б16","К ДА 13 Н","B DAL13","BT2","Адрес-данные","DAL13","АД13",null,"A13",33]
["Б:Б17","К ДА 14 Н","B DAL14","BU2","Адрес-данные","DAL14","АД14",null,"A14",35]
["Б:Б18","К ДА 15 Н","B DAL15","BV2","Адрес-данные","DAL15","АД15",null,"A15",37]
[{"$nulls":6},"A2A1:G77+D42:G77"]

{"sheet":"Лист2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}

{"sheet":"Лист3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}