#### STM32F2x7 ADC Conversion

Home page | Led control | ADC status bar

This page allows you to get continuously the ADC 3 Channel 7 analog input converted value. This ADC Channel is connected to the
STM322xG-EVAL board's potentiometer. The ADC value is updated, automatically, each 1s with the last converted ADC Channel 7 value.
You could check this by changing the potentiometer position and check that the ADC value is updated, by an automatic refresh of this
page, with the new converted value.

ADC Converted Value | mv

###

_______________________________________________________________________________________________________________
All rights reserved © 2016 STMicroelectronics